Arduino

Reference Language | Libraries | Comparison | Changes

LiquidCrystal

## home()

#### Description

Positions the cursor in the upper-left of the LCD. That is, use that location in outputting subsequent text to the display. To also clear the display, use the clear() function instead.

#### Syntax

lcd.home()

#### Parameters

lcd: a variable of type LiquidCrystal

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes