Arduino

Reference Language | Libraries | Comparison | Changes

Keyboard

## Keyboard.println()

#### Description

Sends a keystroke to a connected computer, followed by a newline and carriage return.

Keyboard.println() must be called after initiating Keyboard.begin().

WARNING: When you use the Keyboard.println() command, the Arduino takes over your keyboard! Make sure you have control before you use the command. A pushbutton to toggle the keyboard control state is effective.

#### Syntax

Keyboard.println()
Keyboard.println(character)
Keyboard.println(characters)

#### Parameters

character : a char or int to be sent to the computer as a keystroke, followed by newline and carriage return.
characters : a string to be sent to the computer as a keystroke, followed by a newline and carriage return.

#### Returns

int : number of bytes sent

#### Example

void setup() {
// make pin 2 an input and turn on the
// pullup resistor so it goes high unless
// connected to ground:
pinMode(2, INPUT_PULLUP);
Keyboard.begin();
}
void loop() {
//if the button is pressed
if(digitalRead(2)==LOW){
//Send the message
Keyboard.println("Hello!");
}
}
[Get Code]

#### See Also

- Keyboard.begin()
- Keyboard.end()
- Keyboard.press()
- Keyboard.print()
- Keyboard.release()
- Keyboard.releaseAll()
- Keyboard.write()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes