
adc10_sam3u.o:

adc12_sam3u.o:

adc_sam3snxa.o:

pio.o:
00000000 T PIO_Clear
00000000 T PIO_Configure
00000000 T PIO_DisableInterrupt
00000000 T PIO_Get
00000000 T PIO_GetOutputDataStatus
00000000 T PIO_PullUp
00000000 T PIO_Set
00000000 T PIO_SetDebounceFilter
00000000 T PIO_SetInput
00000000 T PIO_SetOutput
00000000 T PIO_SetPeripheral

pmc.o:
00000000 T pmc_clr_fast_startup_input
00000000 T pmc_disable_all_pck
00000000 T pmc_disable_all_periph_clk
00000000 T pmc_disable_interrupt
00000000 T pmc_disable_pck
00000000 T pmc_disable_periph_clk
00000000 T pmc_disable_pllack
00000000 T pmc_disable_udpck
00000000 T pmc_disable_upll_clock
00000000 T pmc_enable_all_pck
00000000 T pmc_enable_all_periph_clk
00000000 T pmc_enable_backupmode
00000000 T pmc_enable_interrupt
00000000 T pmc_enable_pck
00000000 T pmc_enable_periph_clk
00000000 T pmc_enable_pllack
00000000 T pmc_enable_sleepmode
00000000 T pmc_enable_udpck
00000000 T pmc_enable_upll_clock
00000000 T pmc_enable_waitmode
00000000 T pmc_get_interrupt_mask
00000000 T pmc_get_status
00000000 T pmc_get_writeprotect_status
00000000 T pmc_is_locked_pllack
00000000 T pmc_is_locked_upll
00000000 T pmc_is_pck_enabled
00000000 T pmc_is_periph_clk_enabled
00000000 T pmc_mck_set_prescaler
00000000 T pmc_mck_set_source
00000000 T pmc_osc_disable_fastrc
00000000 T pmc_osc_disable_xtal
00000000 T pmc_osc_enable_fastrc
00000000 T pmc_osc_is_ready_32kxtal
00000000 T pmc_osc_is_ready_mainck
00000000 T pmc_pck_set_prescaler
00000000 T pmc_pck_set_source
00000000 T pmc_set_fast_startup_input
00000000 T pmc_set_writeprotect
00000000 T pmc_switch_mainck_to_fastrc
00000000 T pmc_switch_mainck_to_xtal
00000000 T pmc_switch_mck_to_mainck
00000000 T pmc_switch_mck_to_pllack
00000000 T pmc_switch_mck_to_sclk
00000000 T pmc_switch_mck_to_upllck
00000000 T pmc_switch_pck_to_mainck
00000000 T pmc_switch_pck_to_pllack
00000000 T pmc_switch_pck_to_sclk
00000000 T pmc_switch_pck_to_upllck
00000000 T pmc_switch_sclk_to_32kxtal
00000000 T pmc_switch_udpck_to_pllack
00000000 T pmc_switch_udpck_to_upllck

pwmc.o:
00000000 r C.9.7280
00000000 t FindClockConfiguration
00000000 T PWMC_ConfigureChannel
00000000 T PWMC_ConfigureChannelExt
00000000 T PWMC_ConfigureClocks
00000000 T PWMC_ConfigureComparisonUnit
00000000 T PWMC_ConfigureEventLineMode
00000000 T PWMC_ConfigureSyncChannel
00000000 T PWMC_DisableChannel
00000000 T PWMC_DisableChannelIt
00000000 T PWMC_DisableIt
00000000 T PWMC_DisableOverrideOutput
00000000 T PWMC_EnableChannel
00000000 T PWMC_EnableChannelIt
00000000 T PWMC_EnableFaultProtection
00000000 T PWMC_EnableIt
00000000 T PWMC_EnableOverrideOutput
00000000 T PWMC_FaultClear
00000000 T PWMC_SetDeadTime
00000000 T PWMC_SetDutyCycle
00000000 T PWMC_SetFaultMode
00000000 T PWMC_SetFaultProtectionValue
00000000 T PWMC_SetOverrideValue
00000000 T PWMC_SetPeriod
00000000 T PWMC_SetSyncChannelUpdatePeriod
00000000 T PWMC_SetSyncChannelUpdateUnlock
00000000 T PWMC_WriteBuffer
         U __assert_func
00000000 r __func__.5974
00000000 r __func__.5985
00000000 r __func__.6000
00000000 r __func__.6011
00000000 r __func__.6022
00000000 r __func__.6029
00000000 r __func__.6113
00000000 r __func__.6119

rtc.o:
00000000 T RTC_ClearSCCR
00000000 T RTC_DisableIt
00000000 T RTC_EnableIt
00000000 T RTC_GetDate
00000000 T RTC_GetHourMode
00000000 T RTC_GetSR
00000000 T RTC_GetTime
00000000 T RTC_SetDate
00000000 T RTC_SetDateAlarm
00000000 T RTC_SetHourMode
00000000 T RTC_SetTime
00000000 T RTC_SetTimeAlarm
         U __assert_func
00000000 r __func__.5971
00000000 r __func__.5980
00000000 r __func__.5985

rtt.o:
00000000 T RTT_EnableIT
00000000 T RTT_GetStatus
00000000 T RTT_GetTime
00000000 T RTT_SetAlarm
00000000 T RTT_SetPrescaler
         U __assert_func
00000000 r __func__.5978
00000000 r __func__.5986

spi.o:
00000000 T SPI_Configure
00000000 T SPI_ConfigureNPCS
00000000 T SPI_Disable
00000000 T SPI_DisableIt
00000000 T SPI_Enable
00000000 T SPI_EnableIt
00000000 T SPI_GetStatus
00000000 T SPI_IsFinished
00000000 T SPI_Read
00000000 T SPI_Write
         U pmc_enable_periph_clk

tc.o:
00000000 T TC_Configure
00000000 T TC_FindMckDivisor
00000000 T TC_GetStatus
00000000 T TC_ReadCV
00000000 T TC_SetRA
00000000 T TC_SetRB
00000000 T TC_SetRC
00000000 T TC_Start
00000000 T TC_Stop
         U __assert_func
00000000 r __func__.5973
00000000 r __func__.5979
00000000 r __func__.5985

timetick.o:
00000000 T GetTickCount
00000000 T Sleep
00000000 T TimeTick_Configure
00000000 T TimeTick_Increment
00000000 T Wait
00000000 b _dwTickCount

twi.o:
00000000 T TWI_ByteReceived
00000000 T TWI_ByteSent
00000000 T TWI_ConfigureMaster
00000000 T TWI_ConfigureSlave
00000000 T TWI_DisableIt
00000000 T TWI_EnableIt
00000000 T TWI_GetMaskedStatus
00000000 T TWI_GetStatus
00000000 T TWI_ReadByte
00000000 T TWI_SendSTOPCondition
00000000 T TWI_StartRead
00000000 T TWI_StartWrite
00000000 T TWI_Stop
00000000 T TWI_TransferComplete
00000000 T TWI_WriteByte
         U __assert_func
00000000 r __func__.6346
00000000 r __func__.6361
00000000 r __func__.6365
00000000 r __func__.6372
00000000 r __func__.6376
00000000 r __func__.6381
00000000 r __func__.6389
00000000 r __func__.6403
00000000 r __func__.6408
00000000 r __func__.6412
00000000 r __func__.6417
00000000 r __func__.6421

usart.o:
00000000 T USART_Configure
00000000 T USART_DisableIt
00000000 T USART_EnableIt
00000000 T USART_GetChar
00000000 T USART_GetStatus
00000000 T USART_IsDataAvailable
00000000 T USART_IsRxReady
00000000 T USART_PutChar
00000000 T USART_Read
00000000 T USART_ReadBuffer
00000000 T USART_SetIrdaFilter
00000000 T USART_SetReceiverEnabled
00000000 T USART_SetTransmitterEnabled
00000000 T USART_Write
00000000 T USART_WriteBuffer
         U __assert_func
00000000 r __func__.6267

wdt.o:
00000000 T WDT_Disable
00000000 T WDT_Enable
00000000 T WDT_GetPeriod
00000000 T WDT_GetStatus
00000000 T WDT_Restart

system_sam3xa.o:
00000000 D SystemCoreClock
00000000 T SystemCoreClockUpdate
00000000 T SystemInit
00000000 T system_init_flash

startup_sam3xa.o:
         U ADC_Handler
         U BusFault_Handler
         U CAN0_Handler
         U CAN1_Handler
         U DACC_Handler
         U DMAC_Handler
         U DebugMon_Handler
         U EFC0_Handler
         U EFC1_Handler
         U EMAC_Handler
         U HSMCI_Handler
         U HardFault_Handler
         U MemManage_Handler
         U NMI_Handler
         U PIOA_Handler
         U PIOB_Handler
         U PIOC_Handler
         U PIOD_Handler
         U PMC_Handler
         U PWM_Handler
         U PendSV_Handler
         U RSTC_Handler
         U RTC_Handler
         U RTT_Handler
00000000 T Reset_Handler
         U SMC_Handler
         U SPI0_Handler
         U SSC_Handler
         U SUPC_Handler
         U SVC_Handler
         U SysTick_Handler
         U TC0_Handler
         U TC1_Handler
         U TC2_Handler
         U TC3_Handler
         U TC4_Handler
         U TC5_Handler
         U TC6_Handler
         U TC7_Handler
         U TC8_Handler
         U TRNG_Handler
         U TWI0_Handler
         U TWI1_Handler
         U UART_Handler
         U UOTGHS_Handler
         U USART0_Handler
         U USART1_Handler
         U USART2_Handler
         U USART3_Handler
         U UsageFault_Handler
         U WDT_Handler
         U _erelocate
         U _estack
         U _etext
         U _ezero
         U _sfixed
         U _srelocate
         U _szero
00000000 R exception_table
         U main

adc.o:
00000000 T adc_configure_power_save
00000000 T adc_configure_sequence
00000000 T adc_configure_timing
00000000 T adc_configure_trigger
00000000 T adc_disable_all_channel
00000000 T adc_disable_anch
00000000 T adc_disable_channel
00000000 T adc_disable_channel_differential_input
00000000 T adc_disable_channel_input_offset
00000000 T adc_disable_interrupt
00000000 T adc_disable_tag
00000000 T adc_disable_ts
00000000 T adc_enable_all_channel
00000000 T adc_enable_anch
00000000 T adc_enable_channel
00000000 T adc_enable_channel_differential_input
00000000 T adc_enable_channel_input_offset
00000000 T adc_enable_interrupt
00000000 T adc_enable_tag
00000000 T adc_enable_ts
00000000 T adc_get_actual_adc_clock
00000000 T adc_get_channel_status
00000000 T adc_get_channel_value
00000000 T adc_get_comparison_mode
00000000 T adc_get_interrupt_mask
00000000 T adc_get_latest_value
00000000 T adc_get_overrun_status
00000000 T adc_get_pdc_base
00000000 T adc_get_status
00000000 T adc_get_tag
00000000 T adc_get_writeprotect_status
00000000 T adc_init
00000000 T adc_set_bias_current
00000000 T adc_set_channel_input_gain
00000000 T adc_set_comparison_channel
00000000 T adc_set_comparison_mode
00000000 T adc_set_comparison_window
00000000 T adc_set_resolution
00000000 T adc_set_writeprotect
00000000 T adc_start
00000000 T adc_start_sequencer
00000000 T adc_stop
00000000 T adc_stop_sequencer

udp.o:

udphs.o:

uotghs.o:
00000000 T UOTGHS_Handler
00000000 B gpf_isr

interrupt_sam_nvic.o:
00000000 D g_interrupt_enabled

uotghs_device.o:
00000000 T UDD_Attach
00000000 T UDD_ClearIN
00000000 T UDD_ClearOUT
00000000 T UDD_ClearSetupInt
00000000 T UDD_Detach
00000000 T UDD_FifoByteCount
00000000 T UDD_GetFrameNumber
00000000 T UDD_Init
00000000 T UDD_InitEP
00000000 T UDD_InitEndpoints
00000000 T UDD_ReadWriteAllowed
00000000 T UDD_ReceivedSetupInt
00000000 T UDD_Recv
00000000 T UDD_Recv8
00000000 T UDD_ReleaseRX
00000000 T UDD_ReleaseTX
00000000 T UDD_Send
00000000 T UDD_Send8
00000000 T UDD_SetAddress
00000000 T UDD_SetStack
00000000 T UDD_Stall
00000000 T UDD_WaitForINOrOUT
00000000 T UDD_WaitIN
00000000 T UDD_WaitOUT
         U g_interrupt_enabled
         U gpf_isr
         U pmc_enable_periph_clk
         U pmc_enable_udpck
         U pmc_enable_upll_clock
         U pmc_switch_udpck_to_upllck
00000000 b ul_recv_fifo_ptr
00000000 b ul_send_fifo_ptr

uotghs_host.o:
00000000 T UHD_BusReset
00000000 T UHD_GetVBUSState
00000000 t UHD_ISR
00000000 T UHD_Init
00000000 T UHD_Pipe0_Alloc
00000000 T UHD_Pipe_Alloc
00000000 T UHD_Pipe_Free
00000000 T UHD_Pipe_Is_Transfer_Complete
00000000 T UHD_Pipe_Read
00000000 T UHD_Pipe_Send
00000000 T UHD_Pipe_Write
00000000 T UHD_SetStack
         U g_interrupt_enabled
         U gpf_isr
         U pmc_enable_periph_clk
         U pmc_enable_udpck
         U pmc_enable_upll_clock
         U pmc_switch_udpck_to_upllck
00000000 b uhd_state

dacc.o:
00000000 T dacc_disable_channel
00000000 T dacc_disable_interrupt
00000000 T dacc_disable_trigger
00000000 T dacc_enable_channel
00000000 T dacc_enable_flexible_selection
00000000 T dacc_enable_interrupt
00000000 T dacc_get_analog_control
00000000 T dacc_get_channel_status
00000000 T dacc_get_interrupt_mask
00000000 T dacc_get_interrupt_status
00000000 T dacc_get_pdc_base
00000000 T dacc_get_writeprotect_status
00000000 T dacc_reset
00000000 T dacc_set_analog_control
00000000 T dacc_set_channel_selection
00000000 T dacc_set_power_save
00000000 T dacc_set_timing
00000000 T dacc_set_transfer_mode
00000000 T dacc_set_trigger
00000000 T dacc_set_writeprotect
00000000 T dacc_write_conversion_data
