Arduino

Reference Language | Libraries | Comparison | Changes

Ethernet : Server class

## println()

#### Description

Print data, followed by a newline, to all the clients connected to a server. Prints numbers as a sequence of digits, each an ASCII character (e.g. the number 123 is sent as the three characters '1', '2', '3').

#### Syntax

server.println()
server.println(data)
server.println(data, BASE)

#### Parameters

data (optional): the data to print (char, byte, int, long, or string)

BASE (optional): the base in which to print numbers: BIN for binary (base 2), DEC for decimal (base 10), OCT for octal (base 8), HEX for hexadecimal (base 16).

#### Returns

byte
println() will return the number of bytes written, though reading that number is optional
Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes