- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_copy_q7.c

Go to the documentation of this file.

    00001 /* ----------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_copy_q7.c
    00009 *
    00010 * Description:  Copies the elements of a Q7 vector.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.7  2010/06/10
    00030 *    Misra-C changes done
    00031 * -------------------------------------------------------------------- */
    00032
    00033 #include "arm_math.h"
    00034
    00053 void arm_copy_q7(
    00054   q7_t * pSrc,
    00055   q7_t * pDst,
    00056   uint32_t blockSize)
    00057 {
    00058   uint32_t blkCnt;                               /* loop counter */
    00059
    00060 #ifndef ARM_MATH_CM0
    00061
    00062   /* Run the below code for Cortex-M4 and Cortex-M3 */
    00063
    00064   /*loop Unrolling */
    00065   blkCnt = blockSize >> 2u;
    00066
    00067   /* First part of the processing with loop unrolling.  Compute 4 outputs at a time.
    00068    ** a second loop below computes the remaining 1 to 3 samples. */
    00069   while(blkCnt > 0u)
    00070   {
    00071     /* C = A */
    00072     /* Copy and then store the results in the destination buffer */
    00073     /* 4 samples are copied and stored at a time using SIMD */
    00074     *__SIMD32(pDst)++ = *__SIMD32(pSrc)++;
    00075
    00076     /* Decrement the loop counter */
    00077     blkCnt--;
    00078   }
    00079
    00080   /* If the blockSize is not a multiple of 4, compute any remaining output samples here.
    00081    ** No loop unrolling is used. */
    00082   blkCnt = blockSize % 0x4u;
    00083
    00084 #else
    00085
    00086   /* Run the below code for Cortex-M0 */
    00087
    00088   /* Loop over blockSize number of values */
    00089   blkCnt = blockSize;
    00090
    00091 #endif /* #ifndef ARM_MATH_CM0 */
    00092
    00093
    00094   while(blkCnt > 0u)
    00095   {
    00096     /* C = A */
    00097     /* Copy and then store the results in the destination buffer */
    00098     *pDst++ = *pSrc++;
    00099
    00100     /* Decrement the loop counter */
    00101     blkCnt--;
    00102   }
    00103 }
    00104

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines